,Width##LENGTH##MILLIMETERS ,URL##OTHER## ,Rim height##LENGTH##MILLIMETERS ,Recessed part offset##LENGTH##MILLIMETERS ,Recessed part height##LENGTH##MILLIMETERS ,Power factor##OTHER## ,Opening width##LENGTH##MILLIMETERS ,Opening length##LENGTH##MILLIMETERS ,Nominal wattage##ELECTRICAL_WATTAGE##WATTS ,Model##OTHER## ,Manufacturer##OTHER## ,Luminous flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS ,Light source offset##LENGTH##MILLIMETERS ,Length##LENGTH##MILLIMETERS ,EAN code##OTHER## ,Default Elevation##LENGTH##MILLIMETERS ,Cover material##OTHER## ,Content version##OTHER## ,Content modified date##OTHER## ,Content creation date##OTHER## ,Color temperature##COLOR_TEMPERATURE##KELVIN ,IES light source##OTHER##
PANEL INDV 600 33 W 3000K ,595 ,https://www.ledvance.com/professional/search?query=4058075201132 ,10 ,12 ,-22 ,0.9 ,580 ,580 ,33 ,PANEL INDV 600 33 W 3000K ,LEDVANCE ,3800 ,2 ,595 ,4058075201132 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,3000 ,IES DATA Panel_IndiviLED : PANEL INDV 600 33 W 3000K
PANEL INDV 600 33 W 4000K ,595 ,https://www.ledvance.com/professional/search?query=4058075201156 ,10 ,12 ,-22 ,0.9 ,580 ,580 ,33 ,PANEL INDV 600 33 W 4000K ,LEDVANCE ,4000 ,2 ,595 ,4058075201156 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV 600 33 W 4000K
PANEL INDV 625 33 W 4000K ,620 ,https://www.ledvance.com/professional/search?query=4058075201194 ,10 ,12 ,-22 ,0.9 ,605 ,605 ,33 ,PANEL INDV 625 33 W 4000K ,LEDVANCE ,4000 ,2 ,620 ,4058075201194 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV 625 33 W 4000K
PANEL INDV 625 DALI 33 W 4000K ,620 ,https://www.ledvance.com/professional/search?query=4058075201279 ,10 ,12 ,-22 ,0.9 ,605 ,605 ,33 ,PANEL INDV 625 DALI 33 W 4000K ,LEDVANCE ,4000 ,2 ,620 ,4058075201279 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV 625 DALI 33 W 4000K
PANEL INDV EM 600 33 W 3000K ,595 ,https://www.ledvance.com/professional/search?query=4058075201293 ,10 ,12 ,-22 ,0.9 ,580 ,580 ,33 ,PANEL INDV EM 600 33 W 3000K ,LEDVANCE ,3800 ,2 ,595 ,4058075201293 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,3000 ,IES DATA Panel_IndiviLED : PANEL INDV EM 600 33 W 3000K
PANEL INDV EM 600 33 W 4000K ,595 ,https://www.ledvance.com/professional/search?query=4058075201316 ,10 ,12 ,-22 ,0.9 ,580 ,580 ,33 ,PANEL INDV EM 600 33 W 4000K ,LEDVANCE ,4000 ,2 ,595 ,4058075201316 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV EM 600 33 W 4000K
PANEL INDV EM 625 33 W 4000K ,620 ,https://www.ledvance.com/professional/search?query=4058075201354 ,10 ,12 ,-22 ,0.9 ,605 ,605 ,33 ,PANEL INDV EM 625 33 W 4000K ,LEDVANCE ,4000 ,2 ,620 ,4058075201354 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV EM 625 33 W 4000K
PANEL INDV 600 33 W 4000K DALI ,595 ,https://www.ledvance.com/professional/search?query=4058075503861 ,10 ,12 ,-22 ,0.9 ,580 ,580 ,33 ,PANEL INDV 600 33 W 4000K DALI ,LEDVANCE ,4000 ,2 ,595 ,4058075503861 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV 600 33 W 4000K DALI
PANEL INDV 600 33 W 3000K DALI ,595 ,https://www.ledvance.com/professional/search?query=4058075503885 ,10 ,12 ,-22 ,0.9 ,580 ,580 ,33 ,PANEL INDV 600 33 W 3000K DALI ,LEDVANCE ,3800 ,2 ,595 ,4058075503885 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,3000 ,IES DATA Panel_IndiviLED : PANEL INDV 600 33 W 3000K DALI
PANEL INDV 625 33 W 3000K DALI ,620 ,https://www.ledvance.com/professional/search?query=4058075503908 ,10 ,12 ,-22 ,0.9 ,605 ,605 ,33 ,PANEL INDV 625 33 W 3000K DALI ,LEDVANCE ,3800 ,2 ,620 ,4058075503908 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,3000 ,IES DATA Panel_IndiviLED : PANEL INDV 625 33 W 3000K DALI
PANEL INDV 625 33 W 4000K DALI ,620 ,https://www.ledvance.com/professional/search?query=4058075503922 ,10 ,12 ,-22 ,0.9 ,605 ,605 ,33 ,PANEL INDV 625 33 W 4000K DALI ,LEDVANCE ,4000 ,2 ,620 ,4058075503922 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV 625 33 W 4000K DALI
PANEL INDV 600 33 W 4000K ZBVR ,595 ,https://www.ledvance.com/professional/search?query=4058075521841 ,10 ,12 ,-22 ,0.9 ,580 ,580 ,33 ,PANEL INDV 600 33 W 4000 K ZBVR ,LEDVANCE ,4000 ,2 ,595 ,4058075521841 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV 600 33W 4000 K ZBVR
PANEL INDV 625 33 W 4000K ZBVR ,620 ,https://www.ledvance.com/professional/search?query=4058075521865 ,10 ,12 ,-22 ,0.9 ,605 ,605 ,33 ,PANEL INDV 625 33 W 4000 K ZBVR ,LEDVANCE ,4000 ,2 ,620 ,4058075521865 ,0 ,LEDVANCE polystyrene 90%W ,1 ,10/5/2022 ,10/5/2022 ,4000 ,IES DATA Panel_IndiviLED : PANEL INDV 625 33W 4000 K ZBVR
